Only Vista 64-bit:


1. Press F8 during the boot process to specify additional parameter
2. Disable driver signing
3. Unpack the archive that came bundled with the hardware to a temporary folder
4. Start the Installer
5. Finish installation
6. Plug in SLM-700 and wait for windows to prompt for driver
7. Browse to the temporary folder. Select the folder called "Vista Treiber"

Vista 32-bit:

1. Unpack the archive that came bundled with the hardware to a temporary folder
2. Start the Installer
3. Finish installation
4. Plug in SLM-700 and wait for windows to prompt for driver
5. Browse to the temporary folder. Select the folder called "Vista Treiber"

For all Versions:
 
To prevent Vista-specific database errors, please start the programm (SLM-700) via right click -> run as administrator.
